Next Previous Up Contents
Next: mark
Up: Plotting
Previous: Surface Types

### 8.3 Layer Types

The different plot layers and how to configure them with parameters is given in the following subsections. The layers which may be plotted on a particular surface depend on the plot geometry, so not all of these are available for every plot command.

- 8.3.1 `mark`
- 8.3.2 `size`
- 8.3.3 `sizexy`
- 8.3.4 `xyvector`
- 8.3.5 `xyerror`
- 8.3.6 `xyellipse`
- 8.3.7 `xycorr`
- 8.3.8 `link2`
- 8.3.9 `mark2`
- 8.3.10 `poly4`
- 8.3.11 `mark4`
- 8.3.12 `polygon`
- 8.3.13 `area`
- 8.3.14 `central`
- 8.3.15 `lines`
- 8.3.16 `marks`
- 8.3.17 `yerrors`
- 8.3.18 `xyerrors`
- 8.3.19 `line`
- 8.3.20 `linearfit`
- 8.3.21 `label`
- 8.3.22 `arealabel`
- 8.3.23 `contour`
- 8.3.24 `grid`
- 8.3.25 `fill`
- 8.3.26 `quantile`
- 8.3.27 `histogram`
- 8.3.28 `kde`
- 8.3.29 `knn`
- 8.3.30 `densogram`
- 8.3.31 `gaussian`
- 8.3.32 `function`
- 8.3.33 `skyvector`
- 8.3.34 `skyellipse`
- 8.3.35 `skycorr`
- 8.3.36 `skydensity`
- 8.3.37 `healpix`
- 8.3.38 `skygrid`
- 8.3.39 `xyzvector`
- 8.3.40 `xyzerror`
- 8.3.41 `line3d`
- 8.3.42 `spheregrid`
- 8.3.43 `yerror`
- 8.3.44 `spectrogram`

Next Previous Up Contents
Next: mark
Up: Plotting
Previous: Surface Types

STILTS - Starlink Tables Infrastructure Library Tool Set
Starlink User Note256
STILTS web page: http://www.starlink.ac.uk/stilts/
Author email: m.b.taylor@bristol.ac.uk
Mailing list: topcat-user@jiscmail.ac.uk